**Updating FR125-III to firmware version 2.5.7**

**Date: January 2013**

The firmware upgrade to version 2.5.6 can be performed using the LCD or the serial console cable. The update instructions are outlined below.

The procedure is as follows:

**Step 1:** Make a top level directory on a USB thumbdrive called "BATUpdates".

**Step 2:** Copy recorder.spd\_ii and recorder.spd\_iii into the BATUpdates directory on the thumbdrive.

**Step 3:** Insert the thumbdrive into a **USB** port on the FR125-III.

a. For LCD controller, insert the LCD into the other USB port of the FR125-III

**Step 4:** Start the FR125-III by plugging in the power.

**Step 5:** When the FR125-III completes booting, stop the recorder

a. For LCD controller, navigate to the Status menu and select State as Stopped

b. For console, type:  
 stop

**Step 6:** Start the update

a. For LCD controller, navigate to SW Update then press OK

b. For console, type:  
 update

**Step 7:** Wait for the software update to complete. It takes less than a minute. Once the update is complete the unit will reboot automatically.

Please contact me if you need any help or have questions

Mark Jensen  
Binary Acoustic Technology  
mrj@binaryacoustictech.com

Happy Batting